A C E G H I M O R S T U V

## S

SCError - Class in amlib.ccid
SCError() - Constructor for class amlib.ccid.SCError
setAppContext(Context) - Method in class amlib.hw.HardwareInterface
setPower(int) - Method in class amlib.ccid.Reader
  To set Card Power
setSlot(byte) - Method in class amlib.ccid.Reader
  To set the slot number of Reader
SLE4428Cmd_Read8Bits(int, int, byte[], int[]) - Method in class amlib.ccid.Reader4428
  SLE4428Cmd_Read8Bits read one byte of data without protect bit from the card.
SLE4428Cmd_Read9Bits(int, int, byte[], byte[], int[]) - Method in class amlib.ccid.Reader4428
  SLE4428Cmd_Read9Bits reads data with protect bits from the card.
SLE4428Cmd_Verify1stPSC(byte) - Method in class amlib.ccid.Reader4428
  SLE4428Cmd_Verify1stPSC is used to verify the 1st PSC byte.
SLE4428Cmd_Verify2ndPSC(byte) - Method in class amlib.ccid.Reader4428
  SLE4428Cmd_Verify2ndPSC is used to verify the 2nd PSC byte.
SLE4428Cmd_VerifyPSCAndEraseErrorCounter(byte, byte, int[]) - Method in class amlib.ccid.Reader4428
  SLE4428Cmd_VerifyPSCAndEraseErrorCounter is used to verify the 1st 2nd PSC bytes and erase error counter if the verification is OK.
SLE4428Cmd_WriteEraseWithoutPB(int, byte) - Method in class amlib.ccid.Reader4428
  SLE4428Cmd_WriteEraseWithoutPB writes one byte data without protect bit to the card.
SLE4428Cmd_WriteEraseWithPB(int, byte) - Method in class amlib.ccid.Reader4428
  SLE4428Cmd_WriteEraseWithPB writes one byte data with protect bit to the card.
SLE4428Cmd_WriteErrorCounter(byte) - Method in class amlib.ccid.Reader4428
  SLE4428Cmd_WriteErrorCounter writes error counter to the card.
SLE4428Cmd_WritePBWithDataComparison(int, byte) - Method in class amlib.ccid.Reader4428
  SLE4428Cmd_WritePBWithDataComparison writes protect bit with data comparison.
SLE4442Cmd_CompareVerificationData(byte, byte) - Method in class amlib.ccid.Reader4442
  SLE4442Cmd_CompareVerificationData compares the data with the specified reference byte in the security memory.
SLE4442Cmd_ReadMainMemory(byte, byte, byte[], int[]) - Method in class amlib.ccid.Reader4442
  SLE4442Cmd_ReadMainMemory reads data from the main memory of the card.
SLE4442Cmd_ReadProtectionMemory(byte, byte[], int[]) - Method in class amlib.ccid.Reader4442
  SLE4442Cmd_ReadProtectionMemory reads data from the protection memory of the card.
SLE4442Cmd_ReadSecurityMemory(byte, byte[], int[]) - Method in class amlib.ccid.Reader4442
  SLE4442Cmd_ReadSecurityMemory reads data from the security memory of the card.
SLE4442Cmd_UpdateMainMemory(byte, byte) - Method in class amlib.ccid.Reader4442
  SLE4442Cmd_UpdateMainMemory updates one byte data in the main memory of the card.
SLE4442Cmd_UpdateSecurityMemory(byte, byte) - Method in class amlib.ccid.Reader4442
  SLE4442CmdUpdateSecurityMemory updates one byte data in the main memory of the card.
SLE4442Cmd_Verify(int, byte[]) - Method in class amlib.ccid.Reader4442
  SLE4442Cmd_Verify Verify the pin of the card.
SLE4442Cmd_WriteProtectionMemory(byte, byte) - Method in class amlib.ccid.Reader4442
  SLE4442CmdWriteProtectionMemory write one byte data in the protection memory of the card.
SLE6636Cmd_Authentication(byte, byte, byte, byte[], byte, byte[], int[]) - Method in class amlib.ccid.Reader6636
  SLE6636Cmd_Authentication send authentication command
SLE6636Cmd_ReadCounters(byte, byte[], int[]) - Method in class amlib.ccid.Reader6636
  The SLE6636Cmd_ReadCounters function read Counter Area from the card.
SLE6636Cmd_ReadMemory(byte, byte, byte, byte[], int[]) - Method in class amlib.ccid.Reader6636
  The SLE6636Cmd_ReadMemory function read Memory Area
SLE6636Cmd_Reload(byte, byte, byte[], int[]) - Method in class amlib.ccid.Reader6636
  The SLE6636Cmd_Reload function reload(Erase 8 Bits with Carry Operation) .
SLE6636Cmd_Verification(byte, byte, byte, byte, byte[], int[]) - Method in class amlib.ccid.Reader6636
  The SLE6636Cmd_Verification function
SLE6636Cmd_WriteCounter(byte, byte, byte, byte[], int[]) - Method in class amlib.ccid.Reader6636
  The SLE6636Cmd_WriteCounter function write Counter Area to the card.
SLE6636Cmd_WriteMemory(int, byte, byte, byte[], byte, byte[], int[]) - Method in class amlib.ccid.Reader6636
  The SLE6636Cmd_WriteMemory function write Memory Area
SLOT_STATUS_CARD_ABSENT - Static variable in class amlib.ccid.Reader
SLOT_STATUS_CARD_ACTIVE - Static variable in class amlib.ccid.Reader
SLOT_STATUS_CARD_INACTIVE - Static variable in class amlib.ccid.Reader
STATUS_MASK - Static variable in class amlib.ccid.SCError
switchMode(byte) - Method in class amlib.ccid.Reader
  To switch to different card mode

A C E G H I M O R S T U V